0

16,000

0

2,000

4,000

6,000

8,000

10,000

12,000

14,000

MEAN-DAILY DISCHARGE, IN CFS

0

12,000

0

2,000

4,000

6,000

8,000

10,000

MEAN-DAILY SPECIFIC CONDUCTANCE, IN uS/CM

May June July Aug Sept Oct 1995

CONDUCTANCE AT WEST POINT (RM 51.6)

CONDUCTANCE BELOW POUGHKEEPSIE (IBM, RM 72.3)

HIGH-TIDE CONDUCTANCE AT

POUGHKEEPSIE WTP (RM 77.2)

SALT FRONT (100 mg/L CHLORIDES)

DRINKING WATER STANDARD (250 mg/L CHLORIDES)

FLOW AT GREEN ISLAND DAM

OVERALL FRESHWATER INFLOW--

GREEN ISLAND PLUS 3 LOWER HUDSON TRIBUTARIES (INCL. 73% OF HUDSON D.A.)

PROVISIONAL U.S. GEOLOGICAL SURVEY DATA HUDSON RIVER SPECIFIC CONDUCTANCE AND FRESHWATER INFLOW PERIOD SHOWN MAY 15 TO OCTOBER 18, 1995