08/01/2014

S211-14.docx

|  |
| --- |
| Use on all projects with roadway obliteration. |

## Section 211. — ROADWAY OBLITERATION

**Description**

**211.01 (a) Method 1.** Add the following:

Blend obliteration areas into the adjacent natural ground along the horizontal and vertical planes by gradually transitioning obliteration slopes to remove noticeable breaks.

**Measurement**

**211.05** Add the following:

Do not measure areas within slope stake limits under roadway obliteration.

Measure material excavated from an obliterated roadway and used for new construction or in separate obliteration locations under Section 204.