## Section 106. — Acceptance of Work

11/05/15– FP-14

WFL Specification 11/05/15

Include the following in all projects requiring sampling and testing. Edit as required.

### 106.01 Conformity with Contract Requirements.

Amend as follows:

Add the following to the second paragraph:

Use the modified AASHTO procedures for sampling and testing contained in the WFLHD *Supplements to Nationally Developed Standard Test Procedures*; except, when a specified sampling or test method is not included in this supplement, sample and test according to the referenced AASHTO test procedure.

Delete the third paragraph and substitute the following:

Use the FLH *Field Materials Manual (FMM), Appendix B: FLH Test Methods* in effect on the date of the IFB or RFP. Electronic copies of the FLH Test Methods and FHWA forms can be downloaded from:

<https://flh.fhwa.dot.gov/resources/materials/fmm/>.

Delete the fourteenth paragraph and substitute the following:

Remove, repair, or replace work that does not conform to the contract, or to prevailing industry standards where no specific contract requirements are noted. Removing, repairing, or replacing work; providing temporary traffic control; and any other related work to accomplish conformity will be at no cost to the Government.

WFL Specification 10/01/15

Include the following in all projects.

Add the following:

Obtain copies of the following documents at:

<https://flh.fhwa.dot.gov/resources/construction/paynotes/>

* *Construction Paynote Examples*, dated August 2011.

Obtain copies of the following documents at:

<https://flh.fhwa.dot.gov/business/resources/materials/>

* Appendix B of the *Federal Lands Highway Field Materials Manual*, dated October 2008;
* WFLHD *Supplements to Nationally Developed Standard Test Procedures*;
* Standard WFLHD *Method of Test for Accelerated Weathering of Aggregate by Use of Dimethyl Sulfoxide (DMSO)*;
* Highway Research Board Bulletin No. 319, *The Humphres Method of Granular Soils*, dated 1962; and,
* FLH Addendum to AASHTO T 308 – *Standard Method of Test for Correction Factors for Hot Mix Asphalt (HMA) Containing Recycled Asphalt Pavement (RAP) by the Ignition Method*.

WFL Specification 05/15/15

Include the following on all projects.

### 106.02 Visual Inspection.

Delete the text of this Subsection and substitute the following:

Acceptance is based on visual inspection of the work for compliance with the specific contract requirements. Use prevailing industry standards in the absence of specific contract requirements or tolerances.

WFL Specification 11/04/15

Include the following on all projects.

### 106.03 Certification.

Add the following after the second paragraph:

Obtain required certifications and maintain records of all required certifications according to Subsections 103.04, 153.04, and 155.07.

Submit a completed Form WFLHD 87 *Certification of Compliance* with each material requiring a certification. An electronic version may be found at:

<https://flh.fhwa.dot.gov/resources/construction/forms/wfl/>.

Submit all certifications to the CO unless otherwise specified in the Section ordering the work.

WFL Specification 01/01/14

Include the following on base + options contracts where partial acceptance is permitted.

### 106.07 Partial and Final Acceptance.

Delete paragraph (a) and substitute the following:

**(a) Partial acceptance.** When the Base Schedule, an Option, or any road within an option is completed, a final inspection of that portion of the project may be requested. If the portion is complete and in compliance with the contract, it will be accepted, and the Contractor will be relieved of further responsibility for maintenance of the completed portion. Partial acceptance does not void or alter any of the terms of the contract.