## Section 310. — Cold In-Place Recycled Asphalt Base Course

03/31/16– FP-14

FLH Transmittal No. 1 07/20/15

WFL Specification 03/31/16

Include the following when work is required in this Section.

Material

### 310.02

Amend as follows:

Delete the following from the material list:

Lime 725.03(c)

Add the following to the material list:

Hydraulic cement 701.01

Lime 725.03 (b)

### 310.03 Composition of Mix (JMF). Delete paragraph (d) and substitute the following:

**(d)** Lime or cement content, if required;

### 310.10 Construction Joints.

Delete paragraph (a) and substitute the following:

**(a) Longitudinal joints.** Offset the longitudinal joint of one layer at least 6 inches (150 millimeters) from the joint in the layer immediately below. Make the longitudinal joint in the top layer along the striped centerline of two-lane roadways or at the lane lines of roadways with more than two lanes.

### 310.12 Acceptance.

Delete the third paragraph and substitute the following:

Cement and lime will be evaluated under Subsections 106.02 and 106.03.