$$633.00A

**Section 633. — PERMANENT TRAFFIC CONTROL**

Revised 10 July 2014

*INCLUDE THE FOLLOWING FOR SIGN PANELS (DO NOT DELETE ANY MATERIAL FROM THIS LIST; SPECIFY REQUIRED MATERIAL IN $$633.03C)*

$$633.01A

633.01. Delete the second paragraph and substitute the following:

Sign panels are designated as plywood, aluminum, extruded aluminum, steel, plastic, or fiberglass reinforced plastic.

*INCLUDE THE FOLLOWING FOR SIGNS ON NPS PROJECTS*

$$633.03A

633.03. Add the following after the first sentence:

Furnish signs also meeting the requirements of the National Park Service UniGuide Sign System Manual.

*INCLUDE THE FOLLOWING FOR SIGNS AND/OR POSTS (AND INCLUDE $$633.03C AND/OR $$633.03D). INCLUDE THE FOLLOWING IF $$633.03E IS USED.*

$$633.03B

633.03. Add the following:

*INCLUDE THE FOLLOWING FOR SIGN PANELS IF A SPECIFIC SIGN PANEL MATERIAL IS REQUIRED — DELETE THE HIGHLIGHTED MATERIAL TYPES THAT ARE NOT ACCEPTABLE*

$$633.03C

Furnish plywood, aluminum, extruded aluminum, steel, plastic, or fiberglass reinforced plastic sign panels.

*INCLUDE THE FOLLOWING FOR POSTS IF A SPECIFIC POST MATERIAL IS REQUIRED — DELETE THE HIGHLIGHTED MATERIAL TYPES THAT ARE NOT ACCEPTABLE*

$$633.03D

Furnish wood, aluminum, galvanized steel, or corrosion resistant steel posts.

*INCLUDE THE FOLLOWING FOR SIGNS ON NPS PROJECTS*

$$633.03E

Paint posts, sign supports, and sign panel backs and edges with Benjamin Moore, Moorgard, exterior latex low luster paint, Federal Standard 595B Color No. 20059 (brown), or approved equal.

*INCLUDE THE FOLLOWING FOR OVERHEAD GREEN GUIDE SIGN PANELS*

$$633.05A

633.05. Add the following after the first sentence of the first paragraph:

For all legends on guide signs, use ASTM Type VIII, IX, X, or 3M DG3 retroreflective sheeting.