08/01/14

S629-14.docx

|  |
| --- |
| Use on projects with rolled erosion control products (also known as matting and erosion control blankets) installed on slopes. |

## Section 629. — ROLLED EROSION CONTROL PRODUCTS AND CELLULAR CONFINEMENT SYSTEMS

**Construction Requirements**

**629.05 (a) Slope Installations.** Delete the text and substitute the following:

**(a) Slope Installations.** At the top of the slope, anchor the RECP by using an anchor trench.

**(1) Anchor trench.** Construct a 6- by 6-inch (150- by 150-millimeter) trench. Extend the upslope terminal end of the RECP 36 inches (900 millimeters) past the trench. Use staples on 12-inch (300‑millimeter) centers to fasten the RECP into the trench. Backfill the trench and compact the soil. Secure the terminal end with a single row of staples on 12-inch (300‑millimeter) centers and cover the end with soil. Apply turf establishment to trench.

Securely fasten all RECP to the soil by installing staples according to the manufacturer’s recommendations.