05/12/2015

S710-14\_05122015.docx

|  |
| --- |
| Include subsections below as appropriate. |

## Section 710. — FENCE AND GUARDRAIL

|  |
| --- |
| Include the following when using steel-backed timber guardrail: |

**710.06 Rail Elements.** Add the following:

**(d) Steel-backed log rail.** Delete the second paragraph and substitute the following:

Fabricate steel backing elements according to ASTM A242.