## Section 708. — Plastic Pipe

08/01/14–FP14

WFL Specification 08/01/14

Include the following when underdrain pipe less than or equal to 10 inches (750 millimeters) is required.

### 708.04 Corrugated polyethylene drainage tubing.

Delete the text of this subsection and substitute the following:

Furnish perforated and nonperforated 3- to 10‑inch (75- to 250‑millimeter) diameter tubing conforming to AASHTO M 252, Type C or CP.