$$601.00A

**Section 601.—MINOR CONCRETE STRUCTURES**

Revised 10 July 2014

*INCLUDE THE FOLLOWING IF STATE MIXES ARE ALLOWED*

$$601.03A

601.03. Delete the first sentence and substitute the following:

Conform to Table 601-1 or furnish a concrete mix used locally by either a Federal or State agency for the construction of minor concrete structures, that also meets the minimum 28‑day compressive strength requirement of Table 601-1.